**CAN Bus Specifics**

Schunk Robot is setup for a bus Baudrate of 500kBits/s (Fastest possible Baudrate for Robot 1Mbit/s)

CAN Bus has to be terminated at both ends and only there! Otherwise you wont get anything.

* P-CAN USB-CAN: no termination included
* ESD USB-CAN: no termination included
* CAN-Cable: till now 1 is terminated one is not
* CAN-Ports of the target machine: both are not terminated
* Short black CAN-Cable: terminated on both sides

Only Peack USB-CAN can read the messages sent from the target machine, not the esd one! This means CANreal can’t see messages from the target machine.